
# Flash Android version

​There are some steps to flash the android  version.

1. Please prepare Serial Cable, Double Head USB Cable as below:



2. Connect the JT1 to your PC as below.





3. Type the flash command via SecureCRTPortable tool.

root

icv123


cd /mnt/app

./FlashDevice 1 &

4. After the command takes effect. The JT1's screen will be black.

The Flash tool MultiDownload\_V2.1.exe will also dispaly " READY ".

Note: You can ask our Technical support engineer for the software: MultiDownload\_V2.1.exe. SecureCRTPortable and the flash package.



5.  MultiDownload\_V2.1.exe will display PASS as below  when you finish flash android version.

